DEVICE ID PAYLOAD

STATUS.RAW RESPONSE\_TO

ISF OFFSET

DASH7 PACKET

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 44 | 04 | 87 | 00 | 00 | 20 | 24 | e4c30454ef97b7 | 20 | 40 | 00 | 17 | db079743 | e17a1644 | 1f00 | fa00 | c201 | 4d | b4e54c42 | f7378d40 |

ORIGIN REQUEST ID FILE ID UINT32 CHECKSUM LITTLE ENDIAN FLOAT

D7 HEADER FIFO TOKEN ADDRESSEE\_CTRL ALP OP TYPE LENGTH IN HEX

TEMP LIGHT RH CO2 VOC LAT LONG